(not updated for pcb-rnd yet)

Building PCB for Windows with a MinGW cross-compiler

1) Install a MinGW cross-compiler.
On Debian and derivatives, you can type 'sudo apt-get install mingw32.'.
You can also build your own by using the build script provided by the
MinGW project.

2) Install native (non-cross) dependencies.

* autoconf, automake, libtool, gettext, intltool.
* glib and gtk+.

3) Edit the w32/minipack.conf file to suit your compiler setup.

4) Enter the w32 directory and run ./build_all.

5) Wait while the script fetches and compiles the PCB dependencies and PCB itself.

6) Run the result with wine: wine result/bin/pcb.exe

7) Copy the result directory to a Windows installation (packaging script is not supplied).

