Main | News | People | Events & timeline | pcb-rnd

# pcb-rnd - settings

There are a few minor changes in default settings compared to mainline pcb.

name | description | where to change
--- | --- | ---
layers | the default layer stack is optimized for two sided boards with 3 layers on both sides | edit or replace /usr/share/pcb-rnd/default.pcb
styles & DRC | default styles and DRC settings are optimized for toner transfer | edit or replace /usr/share/pcb-rnd/default.pcb
grid | on startup "enable visible grid" is on and grid is set to 25 mil | change editor/draw_grid in pcb-conf.lht (in system install dir, in user dir) or in project.lht