COMPOSITE_MIDI(7)

NAME
composite_midi - Default MIDI Implementation for Composite

DESCRIPTION

The default MIDI implementation for Composite is a fixed MIDI implementation. Future versions of Composite will allow you to redefine the MIDI implementation, but a default MIDI Implementation will always be provided.

This description of the MIDI implementation only covers the sampler plugin. At this time it does not apply to the composite-gui.

MIDI IMPLEMENTATION
Function | Transmitted | Recognized | Remarks
Basic Channel | NO | 1-16 | Always listens in OMNI mode, will change in future.
Mode | NO | NO |
Note Number | NO | 36-127 | Depends on drum kit.
Note Velocity | NO | 0-127 |
Polyphonic After Touch | NO | NO |
Channel After Touch | NO | NO |
Control Change | 0 | NO | 0-127 | Bank (coarse)
 | 7 | NO | 0(min)-127(max) | Volume (coarse)
 | 32 | NO | 0-127 | Bank (fine)
 | 39 | NO | 0(min)-127(max) | Volume (fine)
 | 120 | NO | 0-127 | All Sound Off (value is ignored)
 | 123 | NO | 0-127 | All Sound Off (value is ignored)
Program Change | NO | 0-127 | User-defined presets, depends on the bank setting (CC #0, 32)
System Exclusive | NO | NO |
System Common | NO | NO |
System Real Time | 0xF8 | NO | NO | Clock Pulse
 | 0xFA | NO | NO | Start
 | 0xFB | NO | NO | Continue
 | 0xFC | NO | NO | Stop
 | 0xFE | NO | NO | Active Sensing
 | 0xFF | NO | YES | System Reset/Panic

SEE ALSO

composite_sampler(1)

AUTHOR

Gabriel M. Beddingfield
    <gabriel@teuton.org>